|  |  |  |
| --- | --- | --- |
| **Sr.#** | **Description** | **Qty.**  **Kgs.** |
| **1** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=6mm), Length= 3 meter | **32** |
| **2** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=8mm), Length= 3 meter | **57** |
| **3** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=10mm), Length= 3 meter | **89** |
| **4** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=12mm), Length= 3 meter | **128** |
| **5** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=16mm), Length= 3 meter | **227** |
| **6** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=20mm), Length= 3 meter | **354** |
| **7** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=25mm), Length= 3 meter | **552** |
| **8** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=30mm), Length= 3 meter | **596** |
| **9** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=35mm), Length= 3 meter | **812** |
| **10** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=40mm), Length= 3 meter | **1135** |
| **11** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=50mm), Length= 3 meter | **221** |
| **12** | **Bronze Alloy C90500**  As per ASTM B505/B505M Rod, (Size: Ф=60mm), Length= 3 meter | **795** |

**Make:** AZO Materials