|  |  |  |
| --- | --- | --- |
| **SR. NO.** | **ITEM DESCRIPTION** | **QTY** |
| 1 | Copper Wire Enameled (Round THERMEX 200, Size SWG 38, Dia 0.152 mm  (THEIC – modified Polyester imide base Coat with a Polyamide-imide, overcoat)) | 200 kg |
| 2 | Copper Wire Enameled (Round THERMEX 200, Size SWG 9, Dia 3.65 mm  (THEIC – modified Polyester imide base Coat with a Polyamide-imide, overcoat)) | 700 kg |