|  |  |  |
| --- | --- | --- |
| **SR. NO.** | **ITEM DESCRIPTION** | **QTY** |
| 1 | Copper Wire Enameled (Round THERMEX 200, Size SWG 30, Dia 0.314 mm  (THEIC – modified Polyester imide base Coat with a Polyamide-imide, overcoat)) | 300 kg |
| 2 | Copper Wire Enameled (Round THERMEX 200, Size SWG 46, Dia 0.06 mm  (THEIC – modified Polyester imide base Coat with a Polyamide-imide, overcoat)) | 50 kg |
| 3 | Copper Wire Enameled (Round THERMEX 200, Size SWG 33, Dia 0.254 mm  (THEIC – modified Polyester imide base Coat with a Polyamide-imide, overcoat)) | 300 kg |