|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **o1. Item name : Seamless Steel Pipe For genaral Process** | | | | |  |  |
| **Manufacturing Standard : ASME B36.10M** | | |  |  |  |  |
| **Material: Cr.Mo ASTM A335 Gr P11** | | |  |  |  |  |
| **PL END , Per picee Pipe Length 6.0 Meter Or 20 feet** | | | |  |  |  |
| **Schedule : 40** | |  |  |  |  |  |
|  |  |  |  |  |  |  |
| **Sl No** | Nominal pipe Size | Unit | Reqired qty | Unite Price | Total Price | Manufacturers  Comments |
| i | 1/2" | Meter | 60 |  |  |  |
| ii | 3/4" | Meter | 240 |  |  |  |
| iii | 1" | Meter | 240 |  |  |  |
| iv | 1 1/2" | Meter | 60 |  |  |  |
| v | 2 " | Meter | 120 |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **o2. Item name : Seamless Steel Pipe For genaral Process** | | | | |  |  |
| **Manufacturing Standard : ASME B36.10M** | | |  |  |  |  |
| **Material: Cr.Mo ASTM A335 Gr P11** | | |  |  |  |  |
| **PL END , Per picee Pipe Length 6.0 Meter Or 20 feet** | | | |  |  |  |
| **Schedule : XS** | |  |  |  |  |  |
|  |  |  |  |  |  |  |
| **Sl No** | **Nominal pipe Size** | **Unit** | **Reqired qty** | **Unite Price** | **Total Price** | Manufacturers  Comments |
| i | 1/2" | Meter | 60 |  |  |  |
| ii | 3/4" | Meter | 120 |  |  |  |
| iii | 1" | Meter | 120 |  |  |  |
| iv | 2" | Meter | 120 |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **o3. Item name : Seamless Carbon Steel Pipe For High temperature service** | | | | | |  |
| **Manufacturing Standard : ASME B36.10M** | | |  |  |  |  |
| **Material: CS ASTM A106 Gr B** | | |  |  |  |  |
| **PL END , Per picee Pipe Length 6.0 Meter Or 20 feet** | | | |  |  |  |
| **Schedule : 160** | |  |  |  |  |  |
|  |  |  |  |  |  |  |
| **Sl No** | **Nominal pipe Size** | **Unit** | **Reqired qty** | **Unite Price** | **Total Price** | Manufacturers  Comments |
| **i** | **1/2"** | **Meter** | **30** |  |  |  |
| **ii** | **3/4"** | **Meter** | **120** |  |  |  |
| **iii** | **1"** | **Meter** | **120** |  |  |  |
| **iv** | **2"** | **Meter** | **60** |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **o4. Item name : Seamless Carbon Steel Pipe For High temperature service** | | | | | |  |
| **Manufacturing Standard : ASME B36.10M** | | |  |  |  |  |
| **Material: CS ASTM A106 Gr B** | | |  |  |  |  |
| **PL END , Per picee Pipe Length 6.0 Meter Or 20 feet** | | | |  |  |  |
| **Schedule : XS** | |  |  |  |  |  |
|  |  |  |  |  |  |  |
| **Sl No** | **Nominal pipe Size** | **Unit** | **Reqired qty** | **Unite Price** | **Total Price** | Manufacturers  Comments |
| i | 1/2" | Meter | 30 |  |  |  |
| ii | 3/4" | Meter | 120 |  |  |  |
| iii | 1" | Meter | 120 |  |  |  |
| iv | 1 1/2" | Meter | 30 |  |  |  |
| V | 2" |  | 60 |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **o5. Item name : Seamless Ferritic Steel Pipe For high temperature services** | | | | | |  |
| **Manufacturing Standard : ASME B36.10M** | | |  |  |  |  |
| **Material: Cr.Mo ASTM A335 Gr P11** | | |  |  |  |  |
| **PL END , Per picee Pipe Length 6.0 Meter Or 20 feet** | | | |  |  |  |
| **Schedule : XXS** | |  |  |  |  |  |
|  |  |  |  |  |  |  |
| **Sl No** | **Nominal pipe Size** | **Unit** | **Reqired qty** | **Unite Price** | **Total Price** | Manufacturers  Comments |
| i | 1/2" | Meter | 30 |  |  |  |
| ii | 3/4" | Meter | 60 |  |  |  |
| iii | 1" | Meter | 60 |  |  |  |
| iv | 2" | Meter | 30 |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **o6. Item name : Seamless Steel Pipe For supperheated steam** | | | | |  |  |
| **Manufacturing Standard : ASME B36.10M** | | |  |  |  |  |
| **Material: Cr.Mo ASTM A335 Gr P22** | | |  |  |  |  |
| **PL END , Per picee Pipe Length 6.0 Meter Or 20 feet** | | | |  |  |  |
| **Schedule : 160** | |  |  |  |  |  |
|  |  |  |  |  |  |  |
| **Sl No** | **Nominal pipe Size** | **Unit** | **Reqired qty** | **Unite Price** | **Total Price** | Manufacturers  Comments |
| i | 1/2" | Meter | 30 |  |  |  |
| ii | 3/4" | Meter | 60 |  |  |  |
| iii | 1" | Meter | 60 |  |  |  |
| iv | 2" | Meter | 30 |  |  |  |
| **o7. Item name : Seamless Steel Pipe For supperheated steam** | | | | |  |  |
| **Manufacturing Standard : ASME B36.10M** | | |  |  |  |  |
| **Material: Cr.Mo ASTM A335 Gr P22** | | |  |  |  |  |
| **PL END , Per picee Pipe Length 6.0 Meter Or 20 feet** | | | |  |  |  |
| **Schedule : XXS** | |  |  |  |  |  |
|  |  |  |  |  |  |  |
| **Sl No** | **Nominal pipe Size** | **Unit** | **Reqired qty** | **Unite Price** | **Total Price** | Manufacturers  Comments |
| i | 3/4" | Meter | 60 |  |  |  |
| ii | 1" | Meter | 60 |  |  |  |
| iii | 2" | Meter | 30 |  |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **o8. Item name : Seamless Steel Pipe For Low temperature service** | | | | | | | | | | |  | |
| **Manufacturing Standard : ASME B36.10M** | | | | |  | |  | |  | |  | |
| **Material: LTS ASTM A333 Gr 6** | | | | |  | |  | |  | |  | |
| **PL END , Per picee Pipe Length 6.0 Meter Or 20 feet** | | | | | | |  | |  | |  | |
| **Schedule : 80** | | |  | |  | |  | |  | |  | |
|  |  | |  | |  | |  | |  | |  | |
| **Sl No** | **Nominal pipe Size** | | **Unit** | | **Reqired qty** | | **Unite Price** | | **Total Price** | | Manufacturers  Comments | |
| i | 1/2" | | Meter | | 30 | |  | |  | |  | |
| ii | 3/4" | | Meter | | 60 | |  | |  | |  | |
| iii | 1" | | Meter | | 60 | |  | |  | |  | |
| iv | 1 1/2" | | Meter | | 30 | |  | |  | |  | |
| v | 2" | |  | | 60 | |  | |  | |  | |
| **o9. Item name : Seamless Steel Pipe For Low temperature service** | | | | | | | | | | | |  | |
| **Manufacturing Standard : ASME B36.10M** | | | | | |  | |  | |  | |  | |
| **Material: LTS ASTM A333 Gr 6** | | | | | |  | |  | |  | |  | |
| **PL END , Per picee Pipe Length 6.0 Meter Or 20 feet** | | | | | | | |  | |  | |  | |
| **Schedule : XXS** | | | |  | |  | |  | |  | |  | |
|  | |  | |  | |  | |  | |  | |  | |
| **Sl No** | | **Nominal pipe Size** | | **Unit** | | **Reqired qty** | | **Unite Price** | | **Total Price** | | Manufacturers  Comments | |
| i | | 1/2" | | Meter | | 30 | |  | |  | |  | |
| ii | | 3/4" | | Meter | | 60 | |  | |  | |  | |
| iii | | 1" | | Meter | | 60 | |  | |  | |  | |
| iv | | 2" | | Meter | | 30 | |  | |  | |  | |
| **\**  **10. Item name : Seamless Steel Pipe For Boiler Feed Water &Steam** | | | | | | | | | | | |  | |
| **Manufacturing Standard : ASME B36.10M** | | | | | |  | |  | |  | |  | |
| **Material: Cr-Mo ASTM A335 Gr P11** | | | | | |  | |  | |  | |  | |
| **PL & BE END , Per picee Pipe Length 6.0 Meter Or 20 feet** | | | | | | | | | |  | |  | |
| **Schedule : 160** | | | |  | |  | |  | |  | |  | |
|  | |  | |  | |  | |  | |  | |  | |
| **Sl No** | | **Nominal pipe Size** | | **Unit** | | **Reqired qty** | | **Unite Price** | | **Total Price** | | Manufacturers  Comments | |
| i | | 1/2" | | Meter | | 30 | |  | |  | |  | |
| ii | | 3/4" | | Meter | | 60 | |  | |  | |  | |
| iii | | 1" | | Meter | | 60 | |  | |  | |  | |
| iv | | 2" | | Meter | | 60 | |  | |  | |  | |