PROJECT TITLE: SUPPLY WITH STEEL RODS

| **NR** | **DESCRIPTION** | **UNIT** | **QUANTITY** | **OFFERED QUANTITY** | **OFFERED PRICE** |
| --- | --- | --- | --- | --- | --- |
| 1. | Shufra rrethore të çelikut, Ø12 x 6000, S235J2, EN 10025-2 | kg | 107 |  |  |
| 2. | Shufra rrethore të çelikut, Ø50 x 6000, S235J2, EN 10025-2 | kg | 1850 |  |  |
| 3. | Shufra rrethore të çelikut, Ø12 x 6000, 42CrMo4, EN 10083-3 | kg | 107 |  |  |
| 4. | Shufra rrethore të çelikut, Ø16 x 6000, 42CrMo4, EN 10083-3 | kg | 190 |  |  |
| 5. | Shufra rrethore të çelikut, Ø20 x 6000, 42CrMo4, EN 10083-3 | kg | 296 |  |  |
| 6. | Shufra rrethore të çelikut, Ø32 x 6000, 42CrMo4, EN 10083-3 | kg | 380 |  |  |
| 7. | Shufra rrethore të çelikut, Ø65 x 6000, 42CrMo4, EN 10083-3 | kg | 1564 |  |  |
| 8. | Shufra rrethore të çelikut, Ø75 x 6000, 42CrMo4, EN 10083-3 | kg | 2100 |  |  |
| 9. | Shufra rrethore të çelikut, Ø80 x 6000, 42CrMo4, EN 10083-3 | kg | 2400 |  |  |
| 10. | Shufra rrethore të çelikut, Ø85 x 6000, 42CrMo4, EN 10083-3 | kg | 2674 |  |  |
| 11. | Shufra rrethore të çelikut, Ø95 x 6000, 42CrMo4, EN 10083-3 | kg | 3340 |  |  |
| 12. | Shufra rrethore të çelikut, Ø100 x 6000, 42CrMo4, EN 10083-3 | kg | 3700 |  |  |
| 13. | Shufra rrethore të çelikut, Ø110 x 6000, 42CrMo4, EN 10083-3 | kg | 2240 |  |  |
| 14. | Shufra rrethore të çelikut, Ø120 x 6000, 42CrMo4, EN 10083-3 | kg | 2664 |  |  |
| 15. | Shufra rrethore të çelikut të përmirësuara 32 ±2 HRC, Ø230 x 3000, 42CrMo4, EN 10083-3 | kg | 5886 |  |  |
| 16. | Shufra rrethore të çelikut të përmirësuara 32 ±2 HRC, Ø370 x 4500, 42CrMo4, EN 10083-3 | kg | 7596 |  |  |

VERY IMPORTANT, PLEASE READ CAREFULLY

Attests of the material for rods in the case of delivery of the material, in the material must be marked the quality of the material and dimensions.

IN CASE OF OFFER, BIDDER IS OBLIGED:

* DECLARATION OF COUNTRY ORIGIN FOR GOODS, IF MORE THAN ONE COUNTRY SPECIFY ALL.
* ISO 9001:2015
* SUPPLY TO KOSOVO FOR 60DAYS
* DECLARATION OF WARRENTY 12MONTHS

*HERE IS A TEMPLATE DECLARATION >>>>>*



Remarks: The tenderer must comply with all the specifications listed in this list. **Any unfulfilled requirement will eliminate the tender in its entirety**. Please check if your tender meets any of the technical specifications described above

Please be aware: Any justification regarding delays due to the COVID 19 Pandemic is and will not be accepted in any circumstance. If the contract is violated, legal actions will be taken from the contracting authority.